## WHEN USING

1. To set Wifi details:

sudo raspi-config

Select the Network Options item from the menu, then the Wi-fi option.

<https://www.raspberrypi.org/documentation/configuration/wireless/wireless-cli.md>

1. To SSH into RPI:

Get IP from router. Ideally setup:

192.168.0.100 for ETHERNET

192.168.0.101 for WiFi b.g

192.168.0.102 for WiFi n

PuTTY with IP of RPi and over SSH port 22

L/P: beo / modern